**Additional information No. 2 to the tender „SUPPLY OF VALVES“ reg.No. VZ 510313**

1. The Contracting Entity has corrected the technical specification TS-A-15GS006/7533. The new version is „TS-A-15GS006/7533 new“.
2. Ball sealing system (item no.23) should be: primary and secondary sealing metal to metal.
3. Correct connection pipe dimension (item no.28) is 60,3 x 4,5 mm.

**Dodatečná informace č. 2 k VZ** **„DODÁVKY ARMATUR“, ev. č. VZ 515138**

1. Zadavatel opravil technickou specifikaci TS-A-15GS006/7533. Nová verze je „TS-A-15GS006/7533 new“.
2. Těsnění (pol. č. 23) musí být primární i sekundární kov-kov.
3. Správné připojení k trubce (pol. č. 28) je 60,3 x 4,5 mm.