**Additional information No. 3 to the tender „SUPPLY OF VALVES“ reg.No. VZ 510313**

1. The Contracting Entity has added the technical specifications for armatures DN 700 PN 63 a DN 500 PN 63 for 1st part BV with metal-to-metal sealing for Dolní Dunajovice UGS: TS-A-15GS008\_7533-Datasheet\_Valves\_DN500 and TS-A-15GS008\_7533-Datasheet\_Valves\_DN500.
2. Bidders can offer fully welded valves only if the specification defines fully welded body of valves.
3. Bidders can offer valves without a wear test certificate (Ruhrgastest) if the tender documentation does not specify that it must be submitted. The same applies for Fire safe test.
4. Bidders cannot offer new designed ball valves without the reference list.

**Dodatečná informace č. 3 k VZ** **„DODÁVKY ARMATUR“, ev. č. VZ 515138**

1. Zadavatel doplnil technické specifikace armatur DN 700 PN 63 a DN 500 PN 63 pro 1. část zakázky KK s těsněním kov - kov pro PZP Dolní Dunajovice: TS-A-15GS008\_7533-Datasheet\_Valves\_DN500 a TS-A-15GS008\_7533-Datasheet\_Valves\_DN500.
2. Uchazeči mohou nabídnout celosvařované armatury pouze pokud specifikace požaduje celosvařované provedení.
3. Uchazeči mohou nabídnout armatury bez testu opotřebení (Ruhrgastest), pokud specifikace nespecifikuje, že musí být předložen. To samé platí pro Fire safe test.
4. Uchazeči nemohou nabídnout nové kulové kohouty bez požadovaných referencí.