# Tools for mechanical works

* Ring wrenches (17, 19, 24, 30mm), in duplicate
* Ring wrenches long type size 24, in duplicate
* Socket wrench set (10 – 32mm), in duplicate
* Screwdrivers for recessed-head screws and slotted screws
* Vise-grip wrench, in duplicate
* Vise, size 1 ½’’, in duplicate
* Hammer (5kg), in duplicate
* Angle-grinder (Ø230mm, 2000W), in duplicate
* Angle-grinder (Ø100mm, 1000W), in duplicate
* Grinding wheels Ø230mm, twenty-fold
* Cut-off wheels Ø230, forty-fold
* Hand drilling machine (chuck Ø15mm, 1000W), in triple
* Twist drills Ø5 – Ø13mm, in duplicate
* Machine screw taps, M6 – M16, in triple
* Cable reel (min. 30m), in triple
* Extension cables (15 – 30m), in quintuplicate
* Pipe-bender, 6 – 12mm
* Welder
* Drill hammer (for M8 – M12)
* HILTI drill hammer (for M12 – M20) and drills Ø20 and Ø25, in triple
* Levelling tool (tolerance +/- 0,5mm at 50m)
* Engineer’s precision level
* Protective barrier