**Attachment No. 2: MEETING TECHNICAL REQUIREMENTS (SPECIFICATION)**

|  |  |
| --- | --- |
| Name of order |  Autoclave for composite material processing (reinforcement)  |
| Type of contract | Machinery equipment delivery  |
| The place of performance of the contract | PRO-CARBON, s.r.o., Loučská 503/31, 75131 Lipník nad Bečvou - Lipník nad Bečvou I-Město |

Company (Supplier) name (including legal form):

Registered office/place of business:

Company registration number:

Tax registration number:

The tenderer shall fill in the table below with the data valid on the day of submitting the offer.

|  |  |
| --- | --- |
| **Required technical parameters**  | **Satisfied / value** |
| Internal useful diameter | Min. 1450 mm |  |
| Internal useful length | Min. 2950 mm |  |
| Internal volume | Min. 10 m3 |  |
| Working pressure | Min. 10 bar |  |
| Max. working temperature | Min. 200°C |  |
| Control board | PLC |  |
| Vacuum automatic indication | Yes |  |

Date \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Signature of the authorized person